|  |  |  |
| --- | --- | --- |
| **FORMEIDF** | **NETWORK RAILEARTHED ISOLATION DETAILS FORM** |  |
|  |  |  |  |  |
| Allocated ref. no. (IPF) | Date and Time | Date and Time | Electrical Risk Assessment Form reference number: | If shared disconnectors are required to be operated, detail individual / company operating below: |
| From | To |  |
| Isolation Instruction issue number: (NP use only) |
|  |  |  |  |  |
| Electrical Section(s) and Subsection(s): | Nominated Person (Level A) | Remarks: |
|  | Name | Company | Sentinel Number |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
| Testing shall be conducted at each earthing location at a minimum of 3 m along the conductor from OLE structures and/or in-line insulation where there is sufficient conductor length. Where 3m is not possible a resistive voltage testing device shall be used. |

|  |  |  |
| --- | --- | --- |
| **Overhead Line Permit along-track limits** |  | **Location of Circuit Main Earths, Additional Earths and Electrical Risk Control Measures** |
| Overhead Line Permit ref. no. | Line / ATF / RC | Structure no. | Line / ATF / RC | Structure Number(At, From-To) | CME / AE / CJ | Residual Electrical Hazard(s) detail  | Type of Electrical Risk Control Measure |
| From | To |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |   |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |

|  |  |
| --- | --- |
| Prepared by: (Nominated Person) | Checked by (Electrical Control Operator) |
| Name  | Signature | Name | Signature |
|  |  |  |  |